GE M90016 SDS


	MOMENTIVE(TM)
INVENTING POSSIBILITIES

SAFETY DATA SHEET

FOR INDUSTRIAL USE ONLY

M90016-30 12C-CRTRG (0.650 LBS-0.295 KG)

	[bookmark: sec0]SECTION 1. PRODUCT AND COMPANY IDENTIFICATION 
	[image: http://complyplus.grainger.com/grainger/images/MSDSText_Top.gif]




PRODUCT NAME: M90016-30 12C-CRTRG (0.650 LBS-0.295 KG)

CHEMICAL NAME: NOT AVAILABLE

MANUFACTURER/IMPORTER/DISTRIBUTOR INFORMATION:
MOMENTIVE AMER SEAL.
260 HUDSON RIVER ROAD
WATERFORD NY 12188

CONTACT PERSON: COMMERCIAL.SERVICES@MOMENTIVE.COM

TELEPHONE:
GENERAL INFORMATION: +1-800-295-2392

EMERGENCY TELEPHONE NUMBER:

SUPPLIER:
CHEMTREC: 1-800-424-9300
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CLASSIFICATION OF THE SUBSTANCE OR MIXTURE:
SKIN CORROSION/IRRITATION: CATEGORY 2
SERIOUS EYE DAMAGE/EYE IRRITATION: CATEGORY 2A
SKIN SENSITIZATION: CATEGORY 1
TOXIC TO REPRODUCTION: CATEGORY 1B
TOXIC TO REPRODUCTION: CATEGORY 1B

GHS LABEL ELEMENTS:

HAZARD PICTOGRAMS:
HEALTH HAZARD
EXCLAMATION MARK

SIGNAL WORD: DANGER

HAZARD STATEMENTS:
H315: CAUSES SKIN IRRITATION.
H319: CAUSES SERIOUS EYE IRRITATION.
H317: MAY CAUSE AN ALLERGIC SKIN REACTION.
H360F: MAY DAMAGE FERTILITY.
H360: MAY DAMAGE THE UNBORN CHILD.

PRECAUTIONARY STATEMENTS:
GENERAL: NOT APPLICABLE.

PREVENTION:
OBTAIN SPECIAL INSTRUCTIONS BEFORE USE.
DO NOT HANDLE UNTIL ALL SAFETY PRECAUTIONS HAVE BEEN READ AND UNDERSTOOD.
USE PERSONAL PROTECTIVE EQUIPMENT AS REQUIRED.
WEAR PROTECTIVE GLOVES.
WEAR EYE OR FACE PROTECTION.
AVOID BREATHING DUST.
WASH HANDS THOROUGHLY AFTER HANDLING.
CONTAMINATED WORK CLOTHING SHOULD NOT BE ALLOWED OUT OF THE WORKPLACE.

RESPONSE:
IF EXPOSED OR CONCERNED: GET MEDICAL ATTENTION.

IF ON SKIN:
WASH WITH PLENTY OF SOAP AND WATER.
TAKE OFF CONTAMINATED CLOTHING.
WASH CONTAMINATED CLOTHING BEFORE REUSE.

IF SKIN IRRITATION OR RASH OCCURS: GET MEDICAL ATTENTION.

IF IN EYES:
RINSE CAUTIOUSLY WITH WATER FOR SEVERAL MINUTES.
REMOVE CONTACT LENSES, IF PRESENT AND EASY TO DO. CONTINUE RINSING.

IF EYE IRRITATION PERSISTS: GET MEDICAL ATTENTION.

STORAGE: STORE LOCKED UP.

DISPOSAL:

P501:
DISPOSE OF CONTENTS AND CONTAINER IN ACCORDANCE WITH ALL LOCAL, REGIONAL,
NATIONAL AND INTERNATIONAL REGULATIONS.

OTHER HAZARDS WHICH DO NOT RESULT IN CLASSIFICATION: NONE KNOWN.
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SUBSTANCE/MIXTURE: MIXTURE

CHEMICAL NAME: NOT AVAILABLE

HAZARDOUS INGREDIENTS                    % BY WEIGHT       CAS NUMBER

OCTAMETHYLCYCLOTETRASILOXANE               1 - 5             556-67-2

SILANAMINE, 1,1,1-TRIMETHYL-               1 - 5             999-97-3
N-(TRIMETHYLSILYL)-

TIN, DIBUTYLBIS(2,4-PENTANEDIONATO-.     0.1 - 1           22673-19-4
KAPPA.O2,.KAPPA.O4)-, (OC-6-11)-

THERE ARE NO ADDITIONAL INGREDIENTS PRESENT WHICH, WITHIN THE CURRENT
KNOWLEDGE OF THE SUPPLIER AND IN THE CONCENTRATIONS APPLICABLE, ARE
CLASSIFIED AS HAZARDOUS TO HEALTH OR THE ENVIRONMENT AND HENCE REQUIRE
REPORTING IN THIS SECTION.

OCCUPATIONAL EXPOSURE LIMITS, IF AVAILABLE, ARE LISTED IN SECTION 8.
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DESCRIPTION OF NECESSARY FIRST AID MEASURES:

EYE CONTACT:
IMMEDIATELY FLUSH EYES WITH PLENTY OF WATER, OCCASIONALLY LIFTING THE UPPER
AND LOWER EYELIDS. CHECK FOR AND REMOVE ANY CONTACT LENSES. CONTINUE TO
RINSE FOR AT LEAST 10 MINUTES. GET MEDICAL ATTENTION.

INHALATION:
REMOVE VICTIM TO FRESH AIR AND KEEP AT REST IN A POSITION COMFORTABLE FOR
BREATHING. IF NOT BREATHING, IF BREATHING IS IRREGULAR OR IF RESPIRATORY
ARREST OCCURS, PROVIDE ARTIFICIAL RESPIRATION OR OXYGEN BY TRAINED
PERSONNEL. IT MAY BE DANGEROUS TO THE PERSON PROVIDING AID TO GIVE
MOUTH-TO-MOUTH RESUSCITATION. GET MEDICAL ATTENTION. IF UNCONSCIOUS, PLACE
IN RECOVERY POSITION AND GET MEDICAL ATTENTION IMMEDIATELY. MAINTAIN AN
OPEN AIRWAY. LOOSEN TIGHT CLOTHING SUCH AS A COLLAR, TIE, BELT OR
WAISTBAND.

SKIN CONTACT:
WASH WITH PLENTY OF SOAP AND WATER. REMOVE CONTAMINATED CLOTHING AND SHOES.
WASH CONTAMINATED CLOTHING THOROUGHLY WITH WATER BEFORE REMOVING IT, OR
WEAR GLOVES. CONTINUE TO RINSE FOR AT LEAST 10 MINUTES. GET MEDICAL
ATTENTION. IN THE EVENT OF ANY COMPLAINTS OR SYMPTOMS, AVOID FURTHER
EXPOSURE. WASH CLOTHING BEFORE REUSE. CLEAN SHOES THOROUGHLY BEFORE REUSE.

INGESTION:
WASH OUT MOUTH WITH WATER. REMOVE DENTURES IF ANY. REMOVE VICTIM TO FRESH
AIR AND KEEP AT REST IN A POSITION COMFORTABLE FOR BREATHING. IF MATERIAL
HAS BEEN SWALLOWED AND THE EXPOSED PERSON IS CONSCIOUS, GIVE SMALL
QUANTITIES OF WATER TO DRINK. STOP IF THE EXPOSED PERSON FEELS SICK AS
VOMITING MAY BE DANGEROUS. DO NOT INDUCE VOMITING UNLESS DIRECTED TO DO SO
BY MEDICAL PERSONNEL. IF VOMITING OCCURS, THE HEAD SHOULD BE KEPT LOW SO
THAT VOMIT DOES NOT ENTER THE LUNGS. GET MEDICAL ATTENTION. NEVER GIVE
ANYTHING BY MOUTH TO AN UNCONSCIOUS PERSON. IF UNCONSCIOUS, PLACE IN
RECOVERY POSITION AND GET MEDICAL ATTENTION IMMEDIATELY. MAINTAIN AN OPEN
AIRWAY. LOOSEN TIGHT CLOTHING SUCH AS A COLLAR, TIE, BELT OR WAISTBAND.

INDICATION OF IMMEDIATE MEDICAL ATTENTION AND SPECIAL TREATMENT NEEDED, IF
NECESSARY:

NOTES TO PHYSICIAN:
IN CASE OF INHALATION OF DECOMPOSITION PRODUCTS IN A FIRE, SYMPTOMS MAY BE
DELAYED. THE EXPOSED PERSON MAY NEED TO BE KEPT UNDER MEDICAL SURVEILLANCE
FOR 48 HOURS.

SPECIFIC TREATMENTS: NO SPECIFIC TREATMENT.

PROTECTION OF FIRST AID PERSONNEL:
NO ACTION SHALL BE TAKEN INVOLVING ANY PERSONAL RISK OR WITHOUT SUITABLE
TRAINING. IF IT IS SUSPECTED THAT FUMES ARE STILL PRESENT, THE RESCUER
SHOULD WEAR AN APPROPRIATE MASK OR SELF-CONTAINED BREATHING APPARATUS.
IT MAY BE DANGEROUS TO THE PERSON PROVIDING AID TO GIVE MOUTH-TO-MOUTH
RESUSCITATION. WASH CONTAMINATED CLOTHING THOROUGHLY WITH WATER BEFORE
REMOVING IT, OR WEAR GLOVES.

SEE TOXICOLOGICAL INFORMATION (SECTION 11)
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EXTINGUISHING MEDIA:

SUITABLE EXTINGUISHING MEDIA:
USE DRY CHEMICAL, CO2, ALCOHOL-RESISTANT FOAM OR WATER SPRAY (FOG).

UNSUITABLE EXTINGUISHING MEDIA: WATER JET

SPECIFIC HAZARDS ARISING FROM THE CHEMICAL:
NO SPECIFIC FIRE OR EXPLOSION HAZARD.

HAZARDOUS THERMAL DECOMPOSITION PRODUCTS:

DECOMPOSITION PRODUCTS MAY INCLUDE THE FOLLOWING MATERIALS:
CARBON DIOXIDE
CARBON MONOXIDE
NITROGEN OXIDES
METAL OXIDE/OXIDES

MEASUREMENTS AT TEMPERATURES ABOVE 150 DEG. C IN PRESENCE OF AIR (OXYGEN)
HAVE SHOWN THAT SMALL AMOUNTS OF FORMALDEHYDE ARE FORMED DUE TO OXIDATIVE
DEGRADATION.

SPECIAL PROTECTIVE ACTIONS FOR FIRE-FIGHTERS:
PROMPTLY ISOLATE THE SCENE BY REMOVING ALL PERSONS FROM THE VICINITY OF
THE INCIDENT IF THERE IS A FIRE. NO ACTION SHALL BE TAKEN INVOLVING ANY
PERSONAL RISK OR WITHOUT SUITABLE TRAINING. USE WATER SPRAY TO KEEP
FIRE-EXPOSED CONTAINERS COOL. FIRE WATER CONTAMINATED WITH THIS MATERIAL
MUST BE CONTAINED AND PREVENTED FROM BEING DISCHARGED TO ANY WATERWAY,
SEWER OR DRAIN.

SPECIAL PROTECTIVE EQUIPMENT FOR FIRE-FIGHTERS:
FIRE-FIGHTERS SHOULD WEAR APPROPRIATE PROTECTIVE EQUIPMENT AND
SELF-CONTAINED BREATHING APPARATUS (SCBA) WITH A FULL FACE-PIECE OPERATED
IN POSITIVE PRESSURE MODE.
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PERSONAL PRECAUTIONS, PROTECTIVE EQUIPMENT AND EMERGENCY PROCEDURES:

FOR NON-EMERGENCY PERSONNEL:
NO ACTION SHALL BE TAKEN INVOLVING ANY PERSONAL RISK OR WITHOUT SUITABLE
TRAINING. EVACUATE SURROUNDING AREAS. KEEP UNNECESSARY AND UNPROTECTED
PERSONNEL FROM ENTERING. DO NOT TOUCH OR WALK THROUGH SPILLED MATERIAL.
PROVIDE ADEQUATE VENTILATION. WEAR APPROPRIATE RESPIRATOR WHEN VENTILATION
IS INADEQUATE. PUT ON APPROPRIATE PERSONAL PROTECTIVE EQUIPMENT.

FOR EMERGENCY RESPONDERS:
IF SPECIALISED CLOTHING IS REQUIRED TO DEAL WITH THE SPILLAGE, TAKE NOTE OF
ANY INFORMATION IN SECTION 8 ON SUITABLE AND UNSUITABLE MATERIALS. SEE ALSO
THE INFORMATION IN "FOR NON-EMERGENCY PERSONNEL".

ENVIRONMENTAL PRECAUTIONS:
AVOID DISPERSAL OF SPILLED MATERIAL AND RUNOFF AND CONTACT WITH SOIL,
WATERWAYS, DRAINS AND SEWERS. INFORM THE RELEVANT AUTHORITIES IF THE
PRODUCT HAS CAUSED ENVIRONMENTAL POLLUTION (SEWERS, WATERWAYS, SOIL
OR AIR).

METHODS AND MATERIAL FOR CONTAINMENT AND CLEANING UP:

SMALL SPILL:
MOVE CONTAINERS FROM SPILL AREA. VACUUM OR SWEEP UP MATERIAL AND PLACE IN A
DESIGNATED, LABELED WASTE CONTAINER. DISPOSE OF VIA A LICENSED WASTE
DISPOSAL CONTRACTOR.

NOTE:
SEE SECTION 1 OF SDS FOR EMERGENCY CONTACT INFORMATION AND SECTION 13 OF
SDS FOR WASTE DISPOSAL.

LARGE SPILL:
MOVE CONTAINERS FROM SPILL AREA. APPROACH RELEASE FROM UPWIND.
PREVENT ENTRY INTO SEWERS, WATER COURSES, BASEMENTS OR CONFINED AREAS.
VACUUM OR SWEEP UP MATERIAL AND PLACE IN A DESIGNATED, LABELED WASTE
CONTAINER. DISPOSE OF VIA A LICENSED WASTE DISPOSAL CONTRACTOR.

NOTE:
SEE SECTION 1 OF SDS FOR EMERGENCY CONTACT INFORMATION AND SECTION 13 OF
SDS FOR WASTE DISPOSAL.
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PRECAUTIONS FOR SAFE HANDLING:

PROTECTIVE MEASURES:
PUT ON APPROPRIATE PERSONAL PROTECTIVE EQUIPMENT (SEE SECTION 8 OF SDS).
PERSONS WITH A HISTORY OF SKIN SENSITIZATION PROBLEMS SHOULD NOT BE
EMPLOYED IN ANY PROCESS IN WHICH THIS PRODUCT IS USED. AVOID EXPOSURE -
OBTAIN SPECIAL INSTRUCTIONS BEFORE USE. AVOID EXPOSURE DURING PREGNANCY.
DO NOT HANDLE UNTIL ALL SAFETY PRECAUTIONS HAVE BEEN READ AND UNDERSTOOD.
DO NOT GET IN EYES OR ON SKIN OR CLOTHING. DO NOT INGEST. USE ONLY WITH
ADEQUATE VENTILATION. KEEP IN THE ORIGINAL CONTAINER OR AN APPROVED
ALTERNATIVE MADE FROM A COMPATIBLE MATERIAL, KEPT TIGHTLY CLOSED WHEN NOT
IN USE. EMPTY CONTAINERS RETAIN PRODUCT RESIDUE AND CAN BE HAZARDOUS.

ADVICE ON GENERAL OCCUPATIONAL HYGIENE:
EATING, DRINKING AND SMOKING SHOULD BE PROHIBITED IN AREAS WHERE THIS
MATERIAL IS HANDLED, STORED AND PROCESSED. WORKERS SHOULD WASH HANDS AND
FACE BEFORE EATING, DRINKING AND SMOKING. SEE ALSO SECTION 8 FOR ADDITIONAL
INFORMATION ON HYGIENE MEASURES.

CONDITIONS FOR SAFE STORAGE, INCLUDING ANY INCOMPATIBILITIES:
STORE IN ACCORDANCE WITH LOCAL REGULATIONS. STORE IN ORIGINAL CONTAINER
PROTECTED FROM DIRECT SUNLIGHT IN A DRY, COOL AND WELL-VENTILATED AREA,
AWAY FROM INCOMPATIBLE MATERIALS (SEE SECTION 10 OF SDS) AND FOOD AND
DRINK. STORE LOCKED UP. KEEP CONTAINER TIGHTLY CLOSED AND SEALED UNTIL
READY FOR USE. CONTAINERS THAT HAVE BEEN OPENED MUST BE CAREFULLY RESEALED
AND KEPT UPRIGHT TO PREVENT LEAKAGE. DO NOT STORE IN UNLABELED CONTAINERS.
USE APPROPRIATE CONTAINMENT TO AVOID ENVIRONMENTAL CONTAMINATION.
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CONTROL PARAMETERS:

OCCUPATIONAL EXPOSURE LIMITS:

INGREDIENT NAME                EXPOSURE LIMITS

OCTAMETHYLCYCLOTETRASILOXANE   ( ) RECOMMENDED EXPOSURE LIMIT (REL): 5 PPM

APPROPRIATE ENGINEERING CONTROLS:
IF USER OPERATIONS GENERATE DUST, FUMES, GAS, VAPOR OR MIST, USE PROCESS
ENCLOSURES, LOCAL EXHAUST VENTILATION OR OTHER ENGINEERING CONTROLS TO KEEP
WORKER EXPOSURE TO AIRBORNE CONTAMINANTS BELOW ANY RECOMMENDED OR STATUTORY
LIMITS.

ENVIRONMENTAL EXPOSURE CONTROLS:
EMISSIONS FROM VENTILATION OR WORK PROCESS EQUIPMENT SHOULD BE CHECKED TO
ENSURE THEY COMPLY WITH THE REQUIREMENTS OF ENVIRONMENTAL PROTECTION
LEGISLATION. IN SOME CASES, FUME SCRUBBERS, FILTERS OR ENGINEERING
MODIFICATIONS TO THE PROCESS EQUIPMENT WILL BE NECESSARY TO REDUCE
EMISSIONS TO ACCEPTABLE LEVELS.

INDIVIDUAL PROTECTION MEASURES:

HYGIENE MEASURES:
WASH HANDS, FOREARMS AND FACE THOROUGHLY AFTER HANDLING CHEMICAL PRODUCTS,
BEFORE EATING, SMOKING AND USING THE LAVATORY AND AT THE END OF THE WORKING
PERIOD. APPROPRIATE TECHNIQUES SHOULD BE USED TO REMOVE POTENTIALLY
CONTAMINATED CLOTHING. CONTAMINATED WORK CLOTHING SHOULD NOT BE ALLOWED OUT
OF THE WORKPLACE. WASH CONTAMINATED CLOTHING BEFORE REUSING. ENSURE THAT
EYEWASH STATIONS AND SAFETY SHOWERS ARE CLOSE TO THE WORKSTATION LOCATION.

EYE/FACE PROTECTION:
SAFETY EYEWEAR COMPLYING WITH AN APPROVED STANDARD SHOULD BE USED WHEN A
RISK ASSESSMENT INDICATES THIS IS NECESSARY TO AVOID EXPOSURE TO LIQUID
SPLASHES, MISTS, GASES OR DUSTS. IF CONTACT IS POSSIBLE, THE FOLLOWING
PROTECTION SHOULD BE WORN, UNLESS THE ASSESSMENT INDICATES A HIGHER DEGREE
OF PROTECTION: CHEMICAL SPLASH GOGGLES.

SKIN PROTECTION:

HAND PROTECTION:
CHEMICAL-RESISTANT, IMPERVIOUS GLOVES COMPLYING WITH AN APPROVED STANDARD
SHOULD BE WORN AT ALL TIMES WHEN HANDLING CHEMICAL PRODUCTS IF A RISK
ASSESSMENT INDICATES THIS IS NECESSARY. CONSIDERING THE PARAMETERS
SPECIFIED BY THE GLOVE MANUFACTURER, CHECK DURING USE THAT THE GLOVES ARE
STILL RETAINING THEIR PROTECTIVE PROPERTIES. IT SHOULD BE NOTED THAT THE
TIME TO BREAKTHROUGH FOR ANY GLOVE MATERIAL MAY BE DIFFERENT FOR DIFFERENT
GLOVE MANUFACTURERS. IN THE CASE OF MIXTURES, CONSISTING OF SEVERAL
SUBSTANCES, THE PROTECTION TIME OF THE GLOVES CANNOT BE ACCURATELY
ESTIMATED.

BODY PROTECTION:
PERSONAL PROTECTIVE EQUIPMENT FOR THE BODY SHOULD BE SELECTED BASED ON THE
TASK BEING PERFORMED AND THE RISKS INVOLVED AND SHOULD BE APPROVED BY A
SPECIALIST BEFORE HANDLING THIS PRODUCT.

OTHER SKIN PROTECTION:
APPROPRIATE FOOTWEAR AND ANY ADDITIONAL SKIN PROTECTION MEASURES SHOULD BE
SELECTED BASED ON THE TASK BEING PERFORMED AND THE RISKS INVOLVED AND
SHOULD BE APPROVED BY A SPECIALIST BEFORE HANDLING THIS PRODUCT.

RESPIRATORY PROTECTION:
USE A PROPERLY FITTED, PARTICULATE FILTER RESPIRATOR COMPLYING WITH AN
APPROVED STANDARD IF A RISK ASSESSMENT INDICATES THIS IS NECESSARY.
RESPIRATOR SELECTION MUST BE BASED ON KNOWN OR ANTICIPATED EXPOSURE LEVELS,
THE HAZARDS OF THE PRODUCT AND THE SAFE WORKING LIMITS OF THE SELECTED
RESPIRATOR.
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APPEARANCE:

PHYSICAL STATE: SOLID

COLOR: COLORLESS.

ODOR: AMMONIA

ODOR THRESHOLD: NOT AVAILABLE

PH: NOT APPLICABLE.

MELTING POINT: NOT APPLICABLE.

BOILING POINT: NOT APPLICABLE.

FLASH POINT: 110.00 DEG. C (230.00 DEG. F) (PENSKY-MARTENS.)

BURNING TIME: NOT AVAILABLE

BURNING RATE: NOT AVAILABLE

EVAPORATION RATE: NOT AVAILABLE

FLAMMABILITY (SOLID, GAS): NOT AVAILABLE

LOWER AND UPPER EXPLOSIVE (FLAMMABLE) LIMITS:
LOWER: NOT APPLICABLE.
UPPER: NOT APPLICABLE.

VAPOR PRESSURE: 1.33 HPA

VAPOR DENSITY: NOT AVAILABLE

RELATIVE DENSITY: 1.03

DENSITY: 1.035 G/CM3

SOLUBILITY: TOLUENE

SOLUBILITY IN WATER: NEGLIGIBLE

PARTITION COEFFICIENT N-OCTANOL/WATER: NOT AVAILABLE

AUTO-IGNITION TEMPERATURE: NOT APPLICABLE.

DECOMPOSITION TEMPERATURE: NOT AVAILABLE

SADT: NOT AVAILABLE

VISCOSITY:
DYNAMIC: NOT AVAILABLE
KINEMATIC: NOT AVAILABLE

VOLATILE ORGANIC CONTENT:
2.8% (W/W)
33 G/L

OTHER INFORMATION: NO ADDITIONAL INFORMATION.
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REACTIVITY: STABLE UNDER NORMAL CONDITIONS.

CHEMICAL STABILITY: THE PRODUCT IS STABLE.

POSSIBILITY OF HAZARDOUS REACTIONS:
UNDER NORMAL CONDITIONS OF STORAGE AND USE, HAZARDOUS REACTIONS WILL NOT
OCCUR.

CONDITIONS TO AVOID: NO SPECIFIC DATA.

INCOMPATIBLE MATERIALS: NO SPECIFIC DATA.

HAZARDOUS DECOMPOSITION PRODUCTS:
UNDER NORMAL CONDITIONS OF STORAGE AND USE, HAZARDOUS DECOMPOSITION
PRODUCTS SHOULD NOT BE PRODUCED.
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INFORMATION ON TOXICOLOGICAL EFFECTS:

ACUTE TOXICITY:

PRODUCT/INGREDIENT NAME   RESULT       SPECIES   DOSE             EXPOSURE

OCTAMETHYLCYCLOTETRA-     LD50 ORAL    RAT       4,800 MG/KG
SILOXANE                                         OECD-GUIDELINE
                                                 401 (ACUTE
                                                 ORAL TOXICITY)

                          LC50         RAT       >12.1 MG/L       4 H
                          INHALATION

                          LC50         RAT       36 MG/L OECD     4 H
                          INHALATION             TEST GUIDELINE
                                                 403

                          LD50 DERMAL  RAT       >2,400 MG/KG
                                                 OECD TEST
                                                 GUIDELINE 402

SILANAMINE,               LD50 ORAL    RAT       850 MG/KG
1,1,1-TRIMETHYL-
N-(TRIMETHYLSILYL)-       LC50         RAT       9 MG/L           4 H
                          INHALATION

CONCLUSION/SUMMARY: NOT DETERMINED

IRRITATION/CORROSION:

PRODUCT/INGREDIENT     RESULT         SPECIES  SCORE  EXPOSURE  OBSERVATION
NAME

OCTAMETHYLCYCLOTETRA-  SKIN           RAT
SILOXANE               OECD-
                       GUIDELINE
                       404 (ACUTE
                       DERMAL
                       IRRITATION/
                       CORROSION)

REMARKS                NON-IRRITATING TO THE SKIN.

                       EYES           RABBIT
                       OECD-
                       GUIDELINE
                       405 (ACUTE
                       EYE
                       IRRITATION/
                       CORROSION)

REMARKS                NON-IRRITATING TO THE EYES.

SILANAMINE,            SKIN           RABBIT
1,1,1-TRIMETHYL-N-     SEVERE
(TRIMETHYLSILYL)-      IRRITANT

CONCLUSION/SUMMARY:
SKIN: NOT DETERMINED
EYES: NOT DETERMINED
RESPIRATORY: NOT DETERMINED

SENSITIZATION:

PRODUCT/INGREDIENT NAME       ROUTE OF    SPECIES      RESULT
                              EXPOSURE
OCTAMETHYLCYCLOTETRASILOXANE              GUINEA PIG   NOT SENSITIZING
                                                       OECD-GUIDELINE 406
                                                       (SKIN SENSITISATION)

CONCLUSION/SUMMARY:
SKIN: NOT DETERMINED
RESPIRATORY: NOT DETERMINED

MUTAGENICITY:

PRODUCT/INGREDIENT NAME        TEST                 EXPERIMENT    RESULT

OCTAMETHYLCYCLOTETRASILOXANE   OECD-GUIDELINE       IN VITRO      NEGATIVE
                               471 (GENETIC
                               TOXICOLOGY:
                               SALMONELLA
                               TYPHIMURIUM,
                               REVERSE MUTATION
                               ASSAY)

                               MOUSE LYMPHOMA       IN VITRO      NEGATIVE
                               ASSAY (OECD
                               GUIDLINE 476)

                               OECD-GUIDELINE       IN VIVO       NEGATIVE
                               474 (GENETIC
                               TOXICOLOGY:
                               MICRONUCLEUS TEST)

CONCLUSION/SUMMARY: NOT DETERMINED

CARCINOGENICITY:

PRODUCT/INGREDIENT NAME   RESULT        SPECIES       DOSE        EXPOSURE

OCTAMETHYLCYCLOTETRA-     INHALATION -  RAT - FEMALE  150 MG/KG   24 MONTHS
SILOXANE                  OECD 453

REMARKS                   NOAEC

                          INHALATION -  RAT - MALE    >700 MG/KG  24 MONTHS
                          OECD 453

REMARKS                   NOAEC

CONCLUSION/SUMMARY: NOT DETERMINED

REPRODUCTIVE TOXICITY:

PRODUCT/     MATERNAL  FERTILITY  DEVELOPMENT  SPECIES  DOSE       EXPOSURE
INGREDIENT   TOXICITY             TOXIN
NAME

OCTAMETHYL-                                    RAT      INHA-
CYCLOTETRA-                                             LATION:
SILOXANE                                                300 MG/KG
                                                        OECD 416

REMARKS      NOAEL PARENTS

                                               RAT      INHA-
                                                        LATION:
                                                        300 MG/KG
                                                        OECD 416

REMARKS      NOAEL F1

CONCLUSION/SUMMARY: NOT DETERMINED

TERATOGENICITY:

PRODUCT/INGREDIENT NAME   RESULT            SPECIES   DOSE        EXPOSURE

OCTAMETHYLCYCLOTETRA-     INHALATION        RABBIT    500 MG/KG   18 DAYS
SILOXANE                  OECD TEST
                          GUIDELINE 414

REMARKS                   NOAEL

                          INHALATION        RABBIT    300 MG/KG   18 DAYS
                          OECD TEST
                          GUIDELINE 414

REMARKS                   NOAEL MATERNITY

CONCLUSION/SUMMARY: NOT DETERMINED

SPECIFIC TARGET ORGAN TOXICITY (SINGLE EXPOSURE):

PRODUCT/INGREDIENT NAME      CATEGORY     ROUTE OF EXPOSURE   TARGET ORGANS

TIN, DIBUTYLBIS(2,4-         CATEGORY 1                       THYMUS
PENTANEDIONATO-.
KAPPA.O2,.KAPPA.O4)-,
(OC-6-11)-

SPECIFIC TARGET ORGAN TOXICITY (REPEATED EXPOSURE):

PRODUCT/INGREDIENT NAME      CATEGORY     ROUTE OF EXPOSURE   TARGET ORGANS

TIN, DIBUTYLBIS(2,4-         CATEGORY 1                       THYMUS
PENTANEDIONATO-.
KAPPA.O2,.KAPPA.O4)-,
(OC-6-11)-

ASPIRATION HAZARD: NOT AVAILABLE

INFORMATION ON THE LIKELY ROUTES OF EXPOSURE: NOT AVAILABLE

POTENTIAL ACUTE HEALTH EFFECTS:

EYE CONTACT: CAUSES SERIOUS EYE IRRITATION.

INHALATION:
EXPOSURE TO DECOMPOSITION PRODUCTS MAY CAUSE A HEALTH HAZARD.
SERIOUS EFFECTS MAY BE DELAYED FOLLOWING EXPOSURE.

SKIN CONTACT: CAUSES SKIN IRRITATION. MAY CAUSE AN ALLERGIC SKIN REACTION.

INGESTION: IRRITATING TO MOUTH, THROAT AND STOMACH.

SYMPTOMS RELATED TO THE PHYSICAL, CHEMICAL AND TOXICOLOGICAL
CHARACTERISTICS:

EYE CONTACT:
ADVERSE SYMPTOMS MAY INCLUDE THE FOLLOWING:
PAIN OR IRRITATION
WATERING
REDNESS

INHALATION:
ADVERSE SYMPTOMS MAY INCLUDE THE FOLLOWING:
REDUCED FETAL WEIGHT
INCREASE IN FETAL DEATHS
SKELETAL MALFORMATIONS

SKIN CONTACT:
ADVERSE SYMPTOMS MAY INCLUDE THE FOLLOWING:
IRRITATION
REDNESS
REDUCED FETAL WEIGHT
INCREASE IN FETAL DEATHS
SKELETAL MALFORMATIONS

INGESTION:
ADVERSE SYMPTOMS MAY INCLUDE THE FOLLOWING:
REDUCED FETAL WEIGHT
INCREASE IN FETAL DEATHS
SKELETAL MALFORMATIONS

DELAYED AND IMMEDIATE EFFECTS AND ALSO CHRONIC EFFECTS FROM SHORT AND LONG
TERM EXPOSURE:

SHORT TERM EXPOSURE:
POTENTIAL IMMEDIATE EFFECTS: NOT AVAILABLE
POTENTIAL DELAYED EFFECTS: NOT AVAILABLE

LONG TERM EXPOSURE:
POTENTIAL IMMEDIATE EFFECTS: NOT AVAILABLE
POTENTIAL DELAYED EFFECTS: NOT AVAILABLE

POTENTIAL CHRONIC HEALTH EFFECTS:

PRODUCT/INGREDIENT NAME         RESULT      SPECIES   DOSE        EXPOSURE

OCTAMETHYLCYCLOTETRASILOXANE    NOAEC       RAT       150 MG/KG   24 MONTHS
                                INHALATION            OECD 453

REMARKS                         NOAEC

                                NOAEL       RABBIT    >1 MG/KG    3 WEEKS

                                DERMAL                OECD 410

REMARKS                         NOAEL

CONCLUSION/SUMMARY: NOT DETERMINED

GENERAL:
ONCE SENSITIZED, A SEVERE ALLERGIC REACTION MAY OCCUR WHEN SUBSEQUENTLY
EXPOSED TO VERY LOW LEVELS.

CARCINOGENICITY: NO KNOWN SIGNIFICANT EFFECTS OR CRITICAL HAZARDS.

MUTAGENICITY: NO KNOWN SIGNIFICANT EFFECTS OR CRITICAL HAZARDS.

TERATOGENICITY: MAY DAMAGE THE UNBORN CHILD.

DEVELOPMENTAL EFFECTS: NO KNOWN SIGNIFICANT EFFECTS OR CRITICAL HAZARDS.

FERTILITY EFFECTS: MAY DAMAGE FERTILITY.

NUMERICAL MEASURES OF TOXICITY:

ACUTE TOXICITY ESTIMATES:

ROUTE                   ATE VALUE

ORAL                    20,650.2 MG/KG

ROUTE                   ATE VALUE

DERMAL                  21,642.6 MG/KG

ROUTE                   ATE VALUE

INHALATION (VAPORS)     793.6 MG/L

OTHER INFORMATION:

OCTAMETHYLCYCLOTETRASILOXANE (D4) INGESTION:
RODENTS GIVEN LARGE DOSES VIA ORAL GAVAGE OF OCTAMETHYLCYCLOTETRASILOXANE
(1600 MG/KG/DAY, 14 DAYS), DEVELOPED INCREASED LIVER WEIGHTS RELATIVE TO
UNEXPOSED CONTROL ANIMALS DUE TO HEPATOCELLULAR HYPERPLASIA (INCREASED
NUMBER OF LIVER CELLS WHICH APPEAR NORMAL) AS WELL AS HYPERTROPHY
(INCREASED CELL SIZE). INHALATION: IN INHALATION STUDIES, LABORATORY
RODENTS EXPOSED TO OCTAMETHYLCYCLOTETRASILOXANE (300 PPM FIVE DAYS/WEEK,
90 DAYS) DEVELOPED INCREASED LIVER WEIGHTS IN FEMALE ANIMALS RELATIVE TO
UNEXPOSED CONTROL ANIMALS. WHEN THE EXPOSURE WAS STOPPED, LIVER WEIGHTS
RETURNED TO NORMAL. MICROSCOPIC EXAMINATION OF THE LIVER CELLS DID NOT SHOW
ANY EVIDENCE OF PATHOLOGY. THIS RESPONSE IN RATS, WHICH DOES NOT AFFECT THE
ANIMAL'S HEALTH, IS WELL-DOCUMENTED AND WIDELY RECOGNIZED. IT IS RELATED TO
AN INCREASE OF LIVER ENZYMES THAT METABOLIZE AND ELIMINATE A MATERIAL FROM
THE BODY. THE INCREASED LIVER WEIGHT REVERSES EVEN WHILE THE D4 EXPOSURE
CONTINUES. THE FINDING IS NOT ADVERSE, BUT IS CONSIDERED A NATURAL ADAPTIVE
CHANGE IN RATS, AND DOES NOT REPRESENT A HAZARD TO HUMANS. INHALATION
STUDIES UTILIZING LABORATORY RABBITS AND GUINEA PIGS SHOWED NO EFFECTS ON
LIVER WEIGHTS. INHALATION EXPOSURES TYPICAL OF INDUSTRIAL USAGE (5-10 PPM)
SHOWED NO TOXIC EFFECTS IN RODENTS. RANGE FINDING REPRODUCTIVE STUDIES WERE
CONDUCTED (WHOLE BODY INHALATION, 70 DAYS PRIOR TO MATING, THROUGH MATING,
GESTATION AND LACTATION), WITH D4. RATS WERE EXPOSED TO 70 AND 700 PPM.
IN THE 700 PPM GROUP, THERE WAS A STATISTICALLY SIGNIFICANT REDUCTION IN
MEAN LITTER SIZE AND IN IMPLANTATION SITES. NO D4 RELATED CLINICAL SIGNS
WERE OBSERVED IN THE PUPS AND NO EXPOSURE RELATED PATHOLOGICAL FINDINGS
WERE FOUND. A TWO-YEAR, COMBINED CHRONIC/CARCINOGENICITY STUDY, DURING
WHICH RATS WERE EXPOSED TO D4 BY INHALATION, DATA SHOWED A STATISTICALLY
SIGNIFICANT INCREASE IN A BENIGN UTERINE TUMOR IN FEMALE RATS EXPOSED AT
THE HIGHEST LEVEL--A LEVEL MUCH HIGHER THAN THE LOW LEVELS THAT CONSUMERS
OR WORKERS MAY ENCOUNTER. AN EXPERT PANEL OF INDEPENDENT SCIENTISTS WHO
HAVE REVIEWED THE RESULTS OF THIS RESEARCH CONCUR THAT THE FINDING SEEN IN
THE TWO-YEAR STUDY OCCURRED THROUGH A BIOLOGICAL PATHWAY THAT IS SPECIFIC
TO THE RAT AND IS NOT RELEVANT TO HUMANS. THEREFORE, THIS OBSERVED EFFECT
DOES NOT INDICATE A POTENTIAL HEALTH HAZARD TO HUMANS. IN DEVELOPMENTAL
TOXICITY STUDIES, RATS AND RABBITS WERE EXPOSED TO D4 AT CONCENTRATIONS UP
TO 700 PPM AND 500 PPM, RESPECTIVELY. NO TERATOGENIC EFFECTS
(BIRTH DEFECTS) WERE OBSERVED IN EITHER STUDY.
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ECOTOXICITY:

CONCLUSION/SUMMARY: NOT AVAILABLE

PERSISTENCE/DEGRADABILITY:

PRODUCT/INGREDIENT         TEST            RESULT         DOSE  INOCULUM
NAME

OCTAMETHYLCYCLOTETRA-    310 READY         3.7 % - 29 D         ACTIVATED
SILOXANE                 BIODEGRADABILITY                       SLUDGE
                         - CO2 IN SEALED
                         VESSELS
                         (HEADSPACE TEST)

REMARKS                  NOT READILY BIODEGRADABLE.

CONCLUSION/SUMMARY: NOT AVAILABLE

BIOACCUMULATIVE POTENTIAL:

PRODUCT/INGREDIENT NAME    SPECIES     EXPOSURE   LOGPOW   BCF    POTENTIAL

OCTAMETHYLCYCLOTETRA-      FATHEAD     28 D                12.40  LOW
SILOXANE                   MINNOW

SILANAMINE, 1,1,1-                                1.19            LOW
TRIMETHYL-N-
(TRIMETHYLSILYL)-

MOBILITY IN SOIL:
SOIL/WATER PARTITION COEFFICIENT (KOC): NOT AVAILABLE
OTHER ADVERSE EFFECTS: NO KNOWN SIGNIFICANT EFFECTS OR CRITICAL HAZARDS.

OTHER INFORMATION:
OCTAMETHYLCYCLOTETRASILOXANE (D4) MEETS THE CURRENT REACH ANNEX XIII
CRITERIA FOR PBT AND VPVB. HOWEVER, D4 DOES NOT BEHAVE SIMILARLY TO KNOWN
PBT/VPVB SUBSTANCES. THE SILICONES INDUSTRIES INTERPRETATION OF THE
AVAILABLE DATA IS THAT THE WEIGHT OF SCIENTIFIC EVIDENCE FROM FIELD STUDIES
SHOWS THAT D4 IS NOT BIOMAGNIFYING IN AQUATIC AND TERRESTRIAL FOOD WEBS.
D4 IN AIR WILL DEGRADE BY REACTION WITH NATURALLY OCCURRING HYDROXYL
RADICALS IN THE ATMOSPHERE. ANY D4 IN AIR THAT DOES NOT DEGRADE BY REACTION
WITH HYDROXYL RADICALS IS NOT EXPECTED TO DEPOSIT FROM THE AIR TO WATER, TO
LAND, OR TO LIVING ORGANISMS.
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DISPOSAL METHODS:
THE GENERATION OF WASTE SHOULD BE AVOIDED OR MINIMIZED WHEREVER POSSIBLE.
DISPOSAL OF THIS PRODUCT, SOLUTIONS AND ANY BY-PRODUCTS SHOULD AT ALL TIMES
COMPLY WITH THE REQUIREMENTS OF ENVIRONMENTAL PROTECTION AND WASTE DISPOSAL
LEGISLATION AND ANY REGIONAL LOCAL AUTHORITY REQUIREMENTS. DISPOSE OF
SURPLUS AND NON-RECYCLABLE PRODUCTS VIA A LICENSED WASTE DISPOSAL
CONTRACTOR. WASTE SHOULD NOT BE DISPOSED OF UNTREATED TO THE SEWER UNLESS
FULLY COMPLIANT WITH THE REQUIREMENTS OF ALL AUTHORITIES WITH JURISDICTION.
WASTE PACKAGING SHOULD BE RECYCLED. INCINERATION OR LANDFILL SHOULD ONLY BE
CONSIDERED WHEN RECYCLING IS NOT FEASIBLE. THIS MATERIAL AND ITS CONTAINER
MUST BE DISPOSED OF IN A SAFE WAY. CARE SHOULD BE TAKEN WHEN HANDLING
EMPTIED CONTAINERS THAT HAVE NOT BEEN CLEANED OR RINSED OUT. EMPTY
CONTAINERS OR LINERS MAY RETAIN SOME PRODUCT RESIDUES. AVOID DISPERSAL OF
SPILLED MATERIAL AND RUNOFF AND CONTACT WITH SOIL, WATERWAYS, DRAINS AND
SEWERS.
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SPECIAL PRECAUTIONS FOR USER:
THIS PRODUCT IS NOT REGARDED AS DANGEROUS GOODS ACCORDING TO THE NATIONAL
AND INTERNATIONAL REGULATIONS ON THE TRANSPORT OF DANGEROUS GOODS.
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UNITED STATES:

U.S. FEDERAL REGULATIONS:
UNITED STATES - TSCA 12(B) - CHEMICAL EXPORT NOTIFICATION: NONE REQUIRED.
UNITED STATES - TSCA 5(A)2 - FINAL SIGNIFICANT NEW USE RULES: NOT LISTED
UNITED STATES - TSCA 5(A)2 - PROPOSED SIGNIFICANT NEW USE RULES: NOT LISTED
UNITED STATES - TSCA 5(E) - SUBSTANCES CONSENT ORDER: NOT LISTED

SARA 311/312:

CLASSIFICATION:
IMMEDIATE (ACUTE) HEALTH HAZARD
DELAYED (CHRONIC) HEALTH HAZARD

CALIFORNIA PROP. 65:

WARNING:
THIS PRODUCT CONTAINS LESS THAN 1% OF A CHEMICAL KNOWN TO THE STATE OF
CALIFORNIA TO CAUSE BIRTH DEFECTS OR OTHER REPRODUCTIVE HARM.

CANADA:

WHMIS (CANADA):
CLASS D-2A: MATERIAL CAUSING OTHER TOXIC EFFECTS (VERY TOXIC).
CLASS D-2B: MATERIAL CAUSING OTHER TOXIC EFFECTS (TOXIC).

INTERNATIONAL REGULATIONS:

INTERNATIONAL LISTS:
AUSTRALIA INVENTORY (AICS): ALL COMPONENTS ARE LISTED OR EXEMPTED.
CANADA INVENTORY: ALL COMPONENTS ARE LISTED OR EXEMPTED.
JAPAN INVENTORY: NOT DETERMINED.
CHINA INVENTORY (IECSC): ALL COMPONENTS ARE LISTED OR EXEMPTED.
KOREA INVENTORY: NOT DETERMINED.
NEW ZEALAND INVENTORY (NZIOC): NOT DETERMINED.
PHILIPPINES INVENTORY (PICCS): NOT DETERMINED.
UNITED STATES INVENTORY (TSCA 8B): ALL COMPONENTS ARE LISTED OR EXEMPTED.
TAIWAN INVENTORY (CSNN): NOT DETERMINED.
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HAZARDOUS MATERIAL INFORMATION SYSTEM III (U.S.A.):
HEALTH           1
FLAMMABILITY     1
PHYSICAL HAZARDS 0

CAUTION:
HMIS(R*) RATINGS ARE BASED ON A 0-4 RATING SCALE, WITH 0 REPRESENTING
MINIMAL HAZARDS OR RISKS, AND 4 REPRESENTING SIGNIFICANT HAZARDS OR RISKS
ALTHOUGH HMIS(R*) RATINGS ARE NOT REQUIRED ON MSDSS UNDER 29 CFR 1910.1200,
THE PREPARER MAY CHOOSE TO PROVIDE THEM. HMIS(R*) RATINGS ARE TO BE USED
WITH A FULLY IMPLEMENTED HMIS(R*) PROGRAM. HMIS(R*) IS A REGISTERED MARK OF
THE NATIONAL PAINT & COATINGS ASSOCIATION (NPCA). HMIS(R*) MATERIALS MAY BE
PURCHASED EXCLUSIVELY FROM J. J. KELLER (800) 327-6868. THE CUSTOMER IS
RESPONSIBLE FOR DETERMINING THE PPE CODE FOR THIS MATERIAL.

FULL TEXT OF ABBREVIATED H STATEMENTS: NOT APPLICABLE.

HISTORY:

DATE OF PRINTING: 02/22/2016

DATE OF ISSUE/DATE OF REVISION: 04/10/2015

DATE OF PREVIOUS ISSUE: 04/03/2015

VERSION: 1.4

PREPARED BY: PRODUCT SAFETY STEWARDSHIP

KEY TO ABBREVIATIONS:

ATE: ACUTE TOXICITY ESTIMATE

BCF: BIOCONCENTRATION FACTOR

GHS:
GLOBALLY HARMONIZED SYSTEM OF CLASSIFICATION AND LABELLING OF CHEMICALS

IATA: INTERNATIONAL AIR TRANSPORT ASSOCIATION

IBC: INTERMEDIATE BULK CONTAINER

IMDG: INTERNATIONAL MARITIME DANGEROUS GOODS

LOGPOW: LOGARITHM OF THE OCTANOL/WATER PARTITION COEFFICIENT

MARPOL 73/78:
INTERNATIONAL CONVENTION FOR THE PREVENTION OF POLLUTION FROM SHIPS, 1973
AS MODIFIED BY THE PROTOCOL OF 1978. ("MARPOL" = MARINE POLLUTION)

RID:
THE REGULATIONS CONCERNING THE INTERNATIONAL CARRIAGE OF DANGEROUS GOODS BY
RAIL

UN: UNITED NATIONS

REFERENCES: NOT AVAILABLE

NOTICE TO READER:
UNLESS OTHERWISE SPECIFIED IN SECTION 1, MOMENTIVE PRODUCTS ARE INTENDED
FOR INDUSTRIAL APPLICATION ONLY. THEY ARE NOT INTENDED FOR SPECIFIC MEDICAL
APPLICATIONS, NEITHER FOR LONG-LASTING (>30 DAYS) IMPLANTATION INTO THE
HUMAN BODY, INJECTED OR DIRECTLY INGESTED, NOR FOR THE MANUFACTURE OF
MULTIPLE USABLE CONTRACEPTIVES KEEP OUT OF THE REACH OF CHILDREN.

FURTHER INFORMATION:
THE INFORMATION PROVIDED IN THIS SAFETY DATA SHEET IS CORRECT TO THE BEST
OF OUR KNOWLEDGE, INFORMATION AND BELIEF AT THE DATE OF ITS PUBLICATION.
THE INFORMATION GIVEN IS DESIGNED ONLY AS A GUIDANCE FOR SAFE HANDLING,
USE, PROCESSING, STORAGE, TRANSPORTATION, DISPOSAL AND RELEASE AND IS NOT
TO BE CONSIDERED A WARRANTY OR QUALITY SPECIFICATION. THE INFORMATION
RELATES ONLY TO THE SPECIFIC MATERIAL DESIGNATED AND MAY NOT BE VALID FOR
SUCH MATERIAL USED IN COMBINATION WITH ANY OTHER MATERIALS OR IN ANY
PROCESS, UNLESS SPECIFIED IN THE TEXT.
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